GRIB2 - GRID TEMPLATE 4.8
Product definition template ― average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval
Created 08/23/2005

Octet | Contents
--- | ---
10 | Parameter category (see Code table 4.1)
11 | Parameter number (see Code table 4.2)
12 | Type of generating process (see Code table 4.3)
13 | Background generating process identifier (defined by originating centre)
14 | Analysis or forecast generating process identified (defined by originating centre)
15-16 | Hours after reference time data cutoff (see Note 1)
17 | Minutes after reference time data cutoff
18 | Indicator of unit of time range (see Code table 4.4)
19-22 | Forecast time in units defined by octet 18 (see Note 2)
23 | Type of first fixed surface (see Code table 4.5)
24 | Scale factor of first fixed surface
25-28 | Scaled value of first fixed surface
29 | Type of second fixed surfaced (see Code table 4.5)
30 | Scale factor of second fixed surface
31-34 | Scaled value of second fixed surfaces
35-36 | Year ― Time of end of overall time interval
37 | Month ― Time of end of overall time interval
38 | Day ― Time of end of overall time interval
39 | Hour ― Time of end of overall time interval
40 | Minute ― Time of end of overall time interval
41 | Second ― Time of end of overall time interval
42 | n ― number of time ranges specifications describing the time intervals used to calculate the statistically-processed field
43-46 | Total number of data values missing in statistical process 47-58 Specification of the outermost (or only) time range over which statistical processing is done
47 | Statistical process used to calculate the processed field from the field at each time increment during the time range (see Code table 4.10)
48 | Type of time increment between successive fields used in the statistical processing (see Code table 4.11)
49 | Indicator of unit of time for time range over which statistical processing is done (see Code table 4.4)
50-53 | Length of the time range over which statistical processing is done, in units defined by the previous octet
54 | Indicator of unit of time for the increment between the successive fields used (see Code table 4.4)
55-58 | Time increment between successive fields, in units defined by the previous octet (see Notes 3 and 4) 59-nn These octets are included only if n>1, where nn = 46 + 12 x n
59-70 | As octets 47 to 58, next innermost step of processing
71-nn | Additional time range specifications, included in accordance with the value of n. Contents as octets 47 to 58, repeated as necessary

Notes: (1) Hours greater than 65534 will be coded as 65534. (2) The reference time in section 1 and the forecast time together define the beginning of the overall time interval. (3) An increment of zero means that the statistical processing the result of continuous (or near continuous) process, not the processing of a number of discrete samples. Examples of such continuous process are the temperatures measured by analogue maximum and minimum thermometers or thermographs and the rainfall measured by a rain gauge. (4) The reference and forecast times are successively set to their initial plus or minus the increment, as defined by the type of time increment (one of octets 48,60,72...). For all but the innermost (last) time range, the next inner range is then processed using these reference and forecast times as the initial reference and forecast time.

Back