GRIB2 - GRID TEMPLATE 3.110
Equatorial azimuthal equidistant projection
Created 8/03/2005

| Contents
--- | ---
15 | Shape of the Earth (see Code table 3.2)
16 | Scale factor of radius of spherical Earth
17-20 | Scaled value of radius of spherical Earth
21 | Scale factor of major axis of oblate of spheroid Earth
22-25 | Scaled value of major axis of oblate spheroid Earth
26 | Scale factor of minor axis of oblate spheroid Earth
27-30 | Scaled value of minor axis of oblate spheroid Earth
31-34 | Nx ― number of points along x-axis
35-38 | Ny ― number of points along y-axis
39-42 | La1 ― latitude of tangency point (centre of grid)
43-46 | Lo1 ― longitude of tangency point
47 | Resolution and component flags (see Flag table 3.3)
48-51 | Dx ― x-direction grid length in units of 10 -3 m as measured at the point of the axis
52-55 | Dy ― y-direction grid length in units of 10-3 m as measured at the point of the axis
56 | Projection centre flag
57 | Scanning mode (see Flag table 3.4)

Back