GRIB2 - GRID TEMPLATE 5.50
Spectral data - simple packing
Created 10/05/2005

Octet | Contents
--- | ---
12-15 | Reference value (R) (IEEE 32-bit floating-point value)
16-17 | Binary scale factor (E)
18-19 | Decimal scale factor (D)
20 | Number of bits used for each packed value (field width)
21-24 | Real part of (0.0) coefficient (IEEE 32-bit floating-point value)

Notes (1) Removal of the real part of (0.0) coefficient from packed data is intended to reduce the variability of the coefficients, in order to improve packing accuracy. (2) For some spectral representations, the (0.0) coefficient represents the mean value of the parameter represented.